Signed-off-by: Zhao Yakui <yakui.zhao@intel.com>
Tested-by: Santi <santi@agolina.net>
---
 drivers/gpu/drm/i915/intel_tv.c |    9 +++++++++
 1 files changed, 9 insertions(+), 0 deletions(-)

diff --git a/drivers/gpu/drm/i915/intel_tv.c b/drivers/gpu/drm/i915/intel_tv.c
index dc83b7a..c8f67bf 100644
--- drivers/gpu/drm/i915/intel_tv.c
+++ drivers/gpu/drm/i915/intel_tv.c
@@ -1267,6 +1267,15 @@
		   DAC_B_0_7_V |
		   DAC_C_0_7_V);

+	/*
+	 * The TV sense state should be cleared to zero on cantiga platform. Otherwise
+	 * the TV is misdetected. This is hardware requirement.
+	 */
+	if (IS_GM45(dev))
+		tv_dac &= ~(TVDAC_STATE_CHG_EN | TVDAC_A_SENSE_CTL |
+			    TVDAC_B_SENSE_CTL | TVDAC_C_SENSE_CTL);
+
+
	I915_WRITE(TV_CTL, tv_ctl);
	I915_WRITE(TV_DAC, tv_dac);
	POSTING_READ(TV_DAC);
