# Template file for 'acpid'
pkgname=acpid
version=2.0.16
revision=2
build_style=gnu-configure
systemd_services="acpid.socket on"
conf_files="/etc/conf.d/acpid"
short_desc="The ACPI Daemon (acpid) With Netlink Support"
maintainer="Juan RP <xtraeme@gmail.com>"
license="GPL-2"
homepage="http://tedfelix.com/linux/acpid-netlink.html"
distfiles="http://tedfelix.com/linux/acpid-$version.tar.xz"
checksum=94df0e73813a5dbaa1d7ae1049b3216b0cfd9d0843c89241080699ca62569808
long_desc="
 In recent linux kernels, the /proc/acpi/event interface has been deprecated.
 The same information (and more) is available via netlink (a way for the kernel
 to communicate with userspace that is usually used for networking) and the
 input layer (mouse, keyboard, power button, etc...). This version of acpid
 supports netlink and the input layer."

post_install() {
	vinstall ${FILESDIR}/acpid.service 644 usr/lib/systemd/system
	vinstall ${FILESDIR}/acpid.socket 644 usr/lib/systemd/system
	vinstall ${FILESDIR}/handler.sh 755 etc/acpi
	vinstall ${FILESDIR}/anything 644 etc/acpi/events
}
